**Setup And Instructions for Ferrocell with LED Ring**

**New! Includes LED controller**. Connect between power supply and 4-pin connector. Tactile buttons change light colors and patterns.

Each **LED is now RGB or W.**

 **Wait 10-30 seconds for the image to manifest. Move magnets position often. Resting magnet in one position for long periods of time may burn the inside surface of the glass, creating a blurred view in the affected area.**

